Aluminum Finishes

* + - * 1. Superior-Performance Organic FEVE Fluoropolymer Powder Finish: Single-coat Fluoropolymer Powder finish complying with AAMA 2605 and containing 100 percent fluorinated ethylene vinyl ether (FEVE) resin. Prepare, pretreat, and apply coating to exposed metal surfaces to comply with coating and resin manufacturers' written instructions.

Color and Gloss: [**As indicated by manufacturer's designations**] [**Match Architect's sample**] [**As selected by Architect from manufacturer's full range**] <**Insert color and gloss**>.

Product code:

Color:

Manufacturer:

Contact:

* + - * 1. High-Performance Organic Super Durable Polyester Powder Finish: Single-coat Super Durable Polyester Powder finish complying with AAMA 2604 and containing super durable polyester resin. Prepare, pretreat, and apply coating to exposed metal surfaces to comply with coating and resin manufacturers' written instructions.

Color and Gloss: [**As indicated by manufacturer's designations**] [**Match Architect's sample**] [**As selected by Architect from manufacturer's full range**] <**Insert color and gloss**>.

Product code:

Color:

Manufacturer:

Contact:

* + - * 1. Powder-Coat Finish at Interior Surfaces: Single-coat Standard Polyester Powder finish complying with AAMA 2603 and containing Standard Polyester resin. Comply with coating manufacturer's written instructions for cleaning, pretreatment, applying and curing finish.

Color and Gloss: [**As indicated by manufacturer's designations**] [**Match Architect's sample**] [**As selected by Architect from manufacturer's full range**] <**Insert color and gloss**>.

Product code:

Color:

Manufacturer:

Contact: